Author: Jason

FEATURES:
Accommodates PVP headsets
Approved as open-face or full-face helmet
Factory Black / White and custom paint colors available
Ultrawide Visor and Pinlock Fog Resistant inner visor
VPS Sun visor with UP 400 Protection
Fits most Intermediate Oval head sizes from XS - 3XL (2 shell sizes)
Air booster ventilation technology
Dual Action Chin Guard opening system
Micro-lock (patented) double lever retention system
Removable/washable “Clima Comfort” interior padding
Eye-wear adaptive system
Blackinton and Smith & Warren badges available upon request
Weight: 3.9 lbs / 1750 grams (approx. for size medium helmet)
5 year limited warranty / Meets or exceeds DOT standards

Nolan Helmet Maintenance and Replacement
Outer Shell - Only commonly available helmet was or plastic cleaning agents should be used to clean any dirt off the helmet’s surface. Apply sparingly to avoid damage.
Plastic Parts Including Shield - Plastic parts should not be cleaned with agents containing solvents. The shield should only be cleaned with water and a neutral cleaning agent. Heavily soiled areas can be gently cleaned using a soft toothbrush or cotton swab.
Liner & Cheek Pads—Should be removed and washed by hand or in washing net in washing machine. Fixed padding should be cleaned with neutral cleaning agent. All parts should be dried in direct sunlight.
Impact Absorption Liner (EPS) - Should be cleaned using only a damp cloth.
Helmet replacement is recommended if the helmet is subjected to an impact, the comfort padding or retention system has become loose, or there are indentations or white scratches in the Impact Absorption Liner (EPS).

SIZE	XSM	SML	MED	LRG	XLG	2XL	3XL

SHELL	XS - MED	LRG - 3XL

HEAD SIZE	55 CM	56 CM	58 CM	60 CM	62 CM	64 CM	65 CM
CHEEK PAD	65MM	60MM	55 MM	50 MM	45 MM	40 MM	35 MM
CENTER PAD	XSM - SML	XSM - SML	MED	LRG	XLG - 2XL	XLG - 2XL	3XL

Replacement Parts and Accessories Available: Sun Visor / Pinlock Shield / Pinlock Lens / Comfort Neck Roll